Conn red-to-blue on RED system 1

authby=secret

auto=route

keyexchange=ikev2

ike=aes128-md5-modp1024

left=192.168.43.130

right=192.168. .

type=transport

esp=aes128-sha-modp1024!